



Department of Corrections and Rehabilitation
Kauai Community Correctional Center
3-5351 Kuhio Highway
Lihue, Kauai, Hawaii 96766

BID ITEM: One (1) 5 Passenger 4-Door Mid-Size Sedan

Specification for 4-door Mid-Size Sedan:
**Plug-in hybrid electric vehicles, currently, the Department of Corrections and Rehabilitation
does not have the necessary infrastructure at its facilities.

The following are the minimum requirements for this vehicle:

1. Model Year:	• 2026 or later ICE vehicle (Internal Combustion Engine) gasoline powered; brand new.

2. Model:	• Mid-Size 4-Door Sedan (5 passengers).

3. Wheelbase:	• 110.0 inches, minimum, 118.0 inches, maximum.

4. Engine:	• Gasoline powered, 
· Fuel rated E-10 or higher, regular unleaded gasoline.

5. Transmission:	• 5-speed automatic minimum, or Continuously Variable Automatic.

6. Steering:	• Variable Power Assisted rack and pinion steering.
7. Brakes:	• Power assisted ventilated front disc, rear drum with ABS.

8. Interior:	• 5 passenger seating capacity (minimum).
· Tilt adjustable steering wheel.
· Dual front (air bags).
· Air Conditioning.
· Front & Rear floor mats.
· Factory gauge package.
· AM/FM Radio.

9. Exterior:	• Remote anti-theft alarm system.
· Remote entry.
· Power door locks.
· Power windows.
· Dual outside mirrors (Powered).

10. Color:	• Neutral tone.

11. Other:	• Three (3) sets of keys.
· Operator's Manual. Electronic format is acceptable.
· Basic warranty 3 yr. / 36000 miles.
· Drivetrain warranty 5 yr. I 60000 miles.
· Corrosion warranty 5 yr. I 60000 miles.

DELIVERY ADDRESS/ AUTHORIZED FACILITY REPRESENTATIVE

Department of Corrections and Rehabilitation
Kauai Community Correctional Center
3-5351 Kuhio Highway
Lihue, HI 96766

	Contact Person: Darlene Afele, (808) 241-3065 or 
			      darlene.a.afele@hawaii.gov



GENERAL SPECIFICATIONS
In addition to detailed specifications herein, the following requirements shall form a part of these specifications:


1. 	Vehicle offered shall include any other standard features not listed but detailed in the manufacturer's brochures and deemed necessary for the proper and safe operation of the vehicle.

2. Manufacturer's standard warranty of 36 months or 36,000 miles and powertrain warranty of 60 months or 60,000 miles from the date the vehicle is placed in service. Full coverage shall include cost of parts, labor and any other expenses incurred in performing warranty work. Warranty documents shall be delivered with the vehicle and shall detail manufacturer's obligation and warranty.

3. Contractor shall provide two copies of the owner-operator manual and service/repair manual at the time the vehicle is delivered. Hard copies are required if available. Electronic version is acceptable provided the electronic version is printable with no material omissions.

4. 	Vehicle shall include and comply with all Federal Motor Vehicle Safety Standards. Vehicle shall also comply with the Code of Federal Regulations, Title 40, Part 85: Control of Air Pollution from New Motor Vehicles and new Motor Vehicle Engines; Environmental Protection Agency.

5. Vehicle shall be completely serviced and in full operational condition upon delivery.

6. 	Accessory or standard equipment installed on the vehicle shall be fully guaranteed by the Contractor against defects resulting from the use of defective or inferior materials or from neglect or from defective workmanship or against all design and manufacturing defects. Warranty period shall begin from the date equipment is placed in service and shall be for a minimum period of one (1) year or for the period guaranteed by the manufacturer, whichever is longer except for rust proofing. Warranty documents shall be delivered with the vehicle and shall detail manufacturer's obligation and warranty procedures. Contractor shall replace or repair defective material and/or workmanship at no cost to the State for parts and labor during the warranty period, provided such defects are not due to abuse or negligence on the part of the State.

7. All equipment offered shall meet ANSI and OSHA safety requirements, and any other Federal or State safety requirements. If applicable or when requested, equipment shall bear a label or written documentation indicating approval of safety requirements from a Bonafide testing laboratory.

8. Manufacturer's standard Corrosion Protection warranty for a minimum of five (5) years, 60,000 miles and warranty documents.

9. MANUALS/TECHNICAL/SERVICE BULLETINS: Successful bidder shall furnish a set of factory service Bulletins: manuals containing system description/service procedures; a set of service special manuals, service labor time, Power train control/emission diagnosis manuals, specified vehicle parts books. All manuals are to be complete and furnished with the delivery of the vehicle. (Electronic format is acceptable).

All technical and service bulletins pertaining to service/repair revisions and identification of new replacement parts from the vehicle manufacturer shall be provided by the successful bidder to KCCC on a timely basis.
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