DAGS/CSD – Window Repairs for 
Kakuhihewa Building (Kapolei SOB) and Keoni Ana
Background
[bookmark: _Hlk180051405]DAGS’s Kakuhihewa Building (Kapolei SOB) and Keoni Ana Building need window repairs.  See attachment Maps and Plans.

Scope of Work
Complete and in place, the following list of repairs.  Notify the Contract Administrator if there are any deviations from the scope of work before proceeding.  Perform all repair work in accordance with the repair material’s instructions.

1. Kakuhihewa Building (Kapolei SOB)

1.1 Reseal all windows on the southwest side (facing the parking lots) of the building:
· Thoroughly clean the area around the window frame.
· Remove the aluminum strips installed around the window frame.
· Apply the sealant described below along the gaps between the window frame and the wall:
· Sikaflex 1A Polyurethane Premium Grade High Performance Elastomeric Sealant, or
· Masterseal SL1 Self-Levelling High Performance Polyurethane Sealant, or approved equal.
· Remove the old sealant from the top of the window flashing and re-seal the joint (refer to drawing 5/A-21 for details).
· Smooth out the sealant with a specialized tool to press the sealant along the gaps between the window frame and the wall.
· Apply the sealant described below along the gaps between the glass and the window frame:
· DOWSIL 795 Silicone Building Sealant
· If any old sealant remains in the gap between the glass and the window frame, it should be removed, and the joint resealed using DOWSIL 795 silicone sealant.
· Smooth out the sealant with a specialized tool to press the sealant along the gaps between the glass and window frame.
· Reinstall the removed aluminum strip using stainless steel screws.

1.2 Reseal all windows on the northwest side (facing Kamokila Blvd) of the building:
· Thoroughly clean the area around the window frame.
· Remove the aluminum strips installed around the window frame.
· Apply the sealant described below along the gaps between the window frame and the wall:
· Sikaflex 1A Polyurethane Premium Grade High Performance Elastomeric Sealant, or
· Masterseal SL1 Self-Levelling High Performance Polyurethane Sealant, or approved equal.
· Remove the old sealant from the top of the window flashing and re-seal the joint (refer to drawing 5/A-21 for details).
· Smooth out the sealant with a specialized tool to press the sealant along the gaps between the window frame and the wall.
· Apply the sealant described below along the gaps between the glass and the window frame:
· DOWSIL 795 Silicone Building Sealant
· If any old sealant remains in the gap between the glass and the window frame, it should be removed, and the joint resealed using DOWSIL 795 silicone sealant.
· Smooth out the sealant with a specialized tool to press the sealant along the gaps between the glass and window frame.
· Reinstall the removed aluminum strip using stainless steel screws.
· Remove all the old caulk on the lower roof and re-caulk the copper flashing.

2. Keoni Ana Building
Replace the cracked window glasses in Room 305 and Room 602:
· Select a glass of the same thickness and type.
· Apply the sealant described below along the gaps between the window frame and the wall:
Sikaflex 1A Polyurethane Premium Grade High Performance Elastomeric Sealant, or
Masterseal SL1 Self-Levelling High Performance Polyurethane Sealant, or approved equal.
· Apply the sealant described below along the gaps between the glass and the window frame:
DOWSIL 795 Silicone Building Sealant
· Smooth out the sealant with a specialized tool to press the sealant along the gaps between the glass and window frame, and the gaps between the window frame and the wall.

3. Clean all repaired windows.

Time of Performance
A. Provide a schedule two (2) weeks after notice to proceed.
B. Twelve (12) months from notice to proceed.
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