
STATE OF HAWAIʻI
DEPARTMENT OF HUMAN RESOURCES DEVELOPMENT
CARPET TILE PRODUCT FORM
DHRD IFB NO. 27-02-ASO

Instructions: Bidders must complete all sections of this form. Provide the specific manufacturer details, product lines, and verify compliance for the proposed carpet tile system. Current manufacturer product literature or technical data sheets must be attached to substantiate compliance, though literature alone does not substitute for completing this form.
1. BIDDER INFORMATION
	Bidder's Legal Business Name:
	

	Authorized Representative Name & Title:
	

	Email Address:
	

	Telephone Number:
	


2. CARPET TILE PRODUCT TECHNICAL SPECIFICATIONS
	Technical Property / Feature
	Minimum Required Specification
	Proposed Product Specification
(Bidder to Complete)

	Manufacturer Name
	Open standard (Commercial grade)
	Brand/Manufacturer: ___________________________

	Product Name & Style
	Open standard (Commercial grade)
	Style Name: ___________________________

	Product Identification / Number
	Open standard
	Product/Style No: ___________________________

	Carpet Tile Size (Nominal)
	Nominally 24 inches × 24 inches
	[  ] 24" × 24"
[  ] Other: ___________________________

	Fiber Type
	Solution-dyed nylon suitable for commercial office use
	[  ] 100% Solution-Dyed Nylon
[  ] Other: ___________________________

	Minimum Face Weight
	Minimum 22 ounces per square yard
	______ oz/sq yd

	Traffic Classification Rating
	Manufacturer-rated for at least Heavy commercial traffic
	[  ] Heavy Commercial
[  ] Severe / Extra Heavy Commercial

	Tuft Density / Construction
	Approx. 6,000 tufts per sq yard or equivalent comparable construction
	Tuft Density: _________________ tufts/sq yd
Construction Type: _____________________

	Backing System Type
	Commercial-grade, manufacturer-approved PVC-free backing system
	[  ] PVC-free Backing
Backing Brand/Type: _____________________

	Indoor Air Quality / VOC (Carpet)
	CRI Green Label Plus requirements or recognized equivalent standard
	[  ] CRI Green Label Plus Compliant
GLP Certification No: _____________________

	Adhesive Low-VOC Standard
	Low-VOC product meeting CRI Green Label Plus or recognized equivalent low-emitting standard
	Adhesive Brand/Model: _____________________
[  ] CRI Green Label Plus Certified

	Transition Materials
	Manufacturer-approved commercial transition profiles to adjacent flooring
	Transition Type/Model: _____________________


3. WARRANTY DOCUMENTATION
	Warranty Component
	Minimum Required Term
	Proposed Warranty Details
(Bidder to Complete)

	Manufacturer Carpet Tile Warranty
	Minimum ten (10) year manufacturer's warranty covering material defects, premature failure, wear, delamination, or backing failure under commercial use.
	Term: __________ Years
[  ] Minimum 10-Yr Warranty Verified

	Adhesive & Transition Warranty
	Manufacturer's standard commercial product warranty.
	[  ] Standard Warranty Included
Term: __________ Years

	Special Flooring Components (Cushion, Underlayment, etc., if applicable)
	Warranted in accordance with written manufacturer documentation; commences upon Phase Acceptance.
	[  ] N/A
[  ] Standard Warranty Included
Term: __________ Years


4. BIDDER CERTIFICATION & SIGN-OFF
By signing below, the Bidder certifies that the carpet tile product and associated materials proposed in this form meet or exceed all technical criteria and warranty terms outlined in Section 5.0 and Section 6.0 of the DHRD IFB No. 27-02-ASO solicitation. The Bidder acknowledges that final color and pattern configurations will be selected by the State post-award from the standard commercial product line of the manufacturer identified herein at no additional cost, and that no product substitutions will be permitted without prior formal written approval from the State.
Authorized Signature: ___________________________          Date: ________________________
Printed Name: _________________________________
Title / Position: _________________________________
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