HAWAII STATE DEPARTMENT OF PUBLIC SAFETY

CORRECTIONS DIVISION
HALAWA CORRECTIONAL FACILITY
HIEPRO SOLICITATION
DRY STANDPIPES AND FIRE HYDRANTS_PHASE III
 BIDS WILL BE RECEIVED UP TO 2:00 P.M. (HST) ON MAY 5, 2023, VIA HIEPRO
The purpose of this Invitation for Bids (IFB) is to establish a contract to:
a) DRY STANDPIPES - Perform annual inspection, testing plus maintenance, and certification with Fire Department Connections:

 2 Each – Medium Security Facility (MSF) 
 2 Each – Special Needs Facility (SNF)
             4 Total

b) FIRE HYDRANTS – Perform annual inspection, testing plus maintenance, and certification with Fire Department Connections:

6 Each – Medium Security Facility (MSF)

2 Each – Special Needs Facility (SNF)


8 Total

Awarded vendor, known as the Contractor, must comply with the terms of the General Conditions. 
In addition, required work shall meet preventive maintenance and inspection service standards of:
1. 29 CFR 1910.158 and NFPA 25 requirements shall be met for Standpipe and Hose Systems.
2. 46 CFR 28.820 and NFPA 291 requirements shall be met for Fire Pumps, Fire Mains, Fire Hydrants, and Fire Hoses.  
The Contractor is responsible for all labor, material, tools, equipment, transportation, and mileage costs necessary to ensure completion of requirements to remove, properly dispose, replace, install, inspect, test, certify, tag, and provide thorough inspection and written reports for fire extinguisher tasks as described in this bid document.
     The services shall be performed at:
      Halawa Correctional Facility
99-902 Moanalua Road

Aiea, Hawai’i 96701
The term of any resulting contract shall begin on May 8, 2023, and end on or        

before June 30, 2023.
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SPECIFICATIONS:

1. All services will comply with NFPA Standards and Contract Manager requirements depending on the type of system. All manufacturer recommendations and any State or local codes will be met.
2. The Contractor will report to the Contract Manager promptly all needed items of maintenance, repairs, and replacement of parts, which in the judgment of the Inspector may be necessary. Requests to repair or replace said parts shall be approved in advance by the Contract Manager prior to any actual work being performed by the Contractor.

3. The Contractor shall maintain or have readily available tools and properly trained personnel to support the fire equipment and system testing and inspections at the Contractor’s cost throughout the duration of the Contract.
4. Payment terms: 100% due within 30 days after satisfactory completion of work invoiced, receipt of the invoice, approval, and acceptance by the Contract Manager.
5. The term of any resulting contract shall begin on May 8, 2023; and end on or before    June 30, 2023.
6. The Contract Manager shall have the right to terminate the contract at any time by giving the Contractor a thirty (30) day written notice.

7. The Contractor is required to report to the Contract Manager or designated representative prior to arriving on facility grounds and reporting out when leaving.
8. The Contractor shall provide only replacement parts that are new and have the same quality and brand name as that being replaced. Substitutions will be permitted only with prior authorization of The Contract Manager or designated representative.

9. All repair services, if required, shall be conducted in full compliance with all specified standards in a manner equal to or better than the normal safety and security procedures 
and standards established by the Contract Manager. At no time shall the facilities or its occupants be placed in jeopardy.

10. All work must be performed in such a manner as not to inconvenience building occupants. The Contractor shall determine the facilities normal working conditions and activities in progress and shall conduct the work in the least disruptive manner.
11. The Contractor shall remove all unused material brought on site and remove and legally dispose of all waste generated by the work.

12. While on property:  a. shirts are required to be always worn, b. no smoking, c. no electronic devices such as radios or headsets.  Exceptions such as a single cell phone or tablet for technical support requires the prior written approval through the Contract Manager.
13. All workers are subject to background security clearances prior to entry, and parking for company vehicles and equipment must be cleared through the Contract Manager.
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A walk-through is not mandatory but will be allowed upon request to the Contract Manager.  A walk-through request must be submitted via email no later than April 27, 2023, to the Contract Manager, Bennett J.A.M. Dias, at bennett.j.dias@hawaii.gov.  The act of submitting a bid is to be considered as full acknowledgment that the bidder inspected the site and is familiar with the conditions and requirements of these specifications.
The bid will be awarded to the lowest responsive, responsible bidder. To be eligible to be awarded any bid over $2,500, a bidder must be “Compliant” with the requirements listed on Hawaii Compliance Express.  To meet this requirement, bidders may either be listed as “Compliant” on Hawaii Compliance Express or produce other documents showing compliance with the requirements listed on Hawaii Compliance Express. These documents must be valid at the time this bid closes. Documents other than the Certificate of Vendor Compliance from Hawaii Compliance Express are subject to verification by the State. Bidders who are NOT compliant at the time this bid closes will not be eligible for the award. 

Any questions regarding the contents of this request can be discussed with the Contract Manager, Bennett J.A.M. Dias, Institutions Facilities Superintendent II, by calling (808) 485-1801 or via email at bennett.j.dias@hawaii.gov.  
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HAWAII STATE DEPARTMENT OF PUBLIC SAFETY

CORRECTIONS DIVISION

HALAWA CORRECTIONAL FACILITY

DRY STANDPIPES AND FIRE HYDRANTS_PHASE III

Company Name:

Address:

Telephone/Facsimile Number:

Email:

The company bid for requested services broken down by service type as follows:
a) DRY STANDPIPES - Perform annual inspection, testing plus maintenance, and certification with Fire Department Connections:

 2 Each – Medium Security Facility (MSF) 

 2 Each – Special Needs Facility (SNF)

             4 Total


$________________________

b) FIRE HYDRANTS – Perform annual inspection, testing plus maintenance, and certification with Fire Department Connections:

6 Each – Medium Security Facility (MSF)

2 Each – Special Needs Facility (SNF)


8 Total

$____________________

Submit as an attachment on HIePRO.
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HAWAII STATE DEPARTMENT OF PUBLIC SAFETY

CORRECTIONS DIVISION

HALAWA CORRECTIONAL FACILITY
DRY STANDPIPES AND FIRE HYDRANTS_PHASE III

Printed Name/Title: _________________________________________________

Signature/Date: ____________________________________________________
This solicitation must be signed by a person authorized to legally bind the bidder.

Submit as an attachment on HIePRO.
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