





ATTACHMENT “B”

Department of Corrections and Rehabilitation
Halawa Correctional Facility Food Service Unit



Invitation for Bids

Notice is hereby given that pursuant to Chapter 103D, Hawaii Revised Statues (HRS), the Department of Corrections and Rehabilitation, Halawa Correctional Facility (HCF) Food Service Unit will be accepting bids to provide one (1) Forklift with a rated capacity of 4000 lbs. at 24” load center. 

The Contractor shall furnish the following:

· (1) Yale Veracitor GC040SVX Series or similar Liquid Propane Gas Forklift.
· (1) Additional 10.2-gallon spare fuel tank.33.5 lb. with Aux. Fill Valve.
· The forklift must have a maximum Outside Turning Radius of less than 79 inches.
· The mast shall be a 3-stage full free lift. 187” max fork height. 
· The forks shall be 42” long Class II Hook type, standard taper. 
· The contractor shall have a minimum of four (4) factory-trained service technicians on Oahu on-call for service calls. 
· The contractor shall have parts in stock in Hawaii for repair of the forklift. If parts are not available in Hawaii, the parts must be available from the factory within 72 hours. 
· The unit shall be delivered to the Halawa Correctional Facility Food Service Unit located at 99-902 Moanalua Road, Aiea, Hawaii 96701.
· The Contractor shall make prior arrangements with the HCF Food Service Manager for delivery date, delivery time, and all applicable clearances.

